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Combination Welder | Ironhill Fabrication and Mechanical, Tulsa, OK 2021 – Present
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EDUCATION

Welding Technology Certificate, Tulsa Tech, 2016

AWS Certified Welder, plate and pipe (current)

ASME Section IX qualifications: GTAW, SMAW, FCAW

KEY SKILLS
· 
Run 6G pipe welds on Sch 80 carbon and 316L stainless for refinery shutdown
projects, hitting a first-time X-ray pass rate of 96% across 217 joints in 2023.
· Set up and weld pressure vessel shells using GTAW root with FCAW fill and cap, working to ASME Section IX procedures.
· Trained 4 helpers on rod control, joint prep, and oven handling; two were promoted to journeyman within 18 months.
· Read isometric drawings to lay out spool work, cutting rework on a 14-line piping package by roughly a third.
· Maintain a clean cert log across SMAW, GTAW, and FCAW on plate and pipe positions 1G through 6G.


Structural Welder | Bluestem Steel Erectors, Wichita, KS 2018 – 2021
· Welded moment connections, beam splices, and column base plates on 4-story commercial frames using FCAW dual shield.
· Passed AWS D1.1 3G and 4G plate tests on first attempt and re-certed annually.

· GTAW (TIG) on stainless, carbon, and aluminum
· SMAW with low-hydrogen rod, 6010/7018
· 
Worked off swing stages and man-lifts to 80 feet with no recordable safety incidents over 3 years.
· Helped layout crew square and shim 62 columns on a hospital expansion ahead of schedule.

· FCAW dual shield and self-shielded

Welder Helper / Fitter | Prairie Tank Works, Enid, OK 2016 – 2018

· 6G pipe, all positions 1G-6GGregory Morris
Welder
AWS-certiﬁed welder with 8 years across structural, pipe, and pressure vessel work. Strong on TIG and GTAW for stainless and carbon steel, with a 96% ﬁrst-pass X-ray rate on the last 200 joints inspected. Comfortable reading ISO drawings, WPS sheets, and running rod ovens on long shutdown jobs.
PROFESSIONAL EXPERIENCE

· Blueprint and ISO drawing reading
· WPS and PQR interpretation
· Rod oven and consumable control
· Plasma cutting, oxy-fuel, track torch
· Confined space and fall protection trained


· Fit and tacked storage tank shells from 20 to 60 ft diameter for ag and oilfield clients.
· Ran SMAW root and hot pass on API 650 floor seams under journeyman supervision.
· Cut and beveled plate on track torch and plasma to within 1/16 in tolerance.
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