Percy Dube
Journeyman Operating Engineer

Operating engineer with 6 years of experience running excavators, bulldozers, front-end loaders, scrapers, and roller compactors on highway, commercial, and residential earthwork projects. Moved an average of 2,740 cubic yards of material per shift on a 4-mile highway realignment and maintained 0 recordable safety incidents over 18 consecutive months. Holds a Commercial Driver's License (Class A) and an A.A.S. in Automotive Systems Technology.




Morganton, NC 12345P R O F E S S I O N A L E X P E R I E N C E


JOURNEYMAN OPERATING ENGINEER
CATAWBA BLUFF GRADING CO., MORGANTON, NC | 2023 – PRESENT


(828) 555-0125


percy.dube@example.com



K E Y S K I L L S

· Excavator Operation
· Bulldozer Operation
· Front-end Loader Operation
· 
Moved an average of 2,740 cubic yards of material per shift operating a front-end loader and scraper on a 4-mile highway realignment project.
· Completed 63 survey hours per quarter staking cut-and-fill sections with the project surveyor, reducing rework delays by 1.5 hours per week.
· Recorded 0 recordable safety incidents over 18 consecutive months by conducting walk-around inspections and enforcing PPE compliance in
active cut zones.
· Drove and maneuvered a bulldozer in successive passes to strip topsoil and distribute select fill across embankment sections spanning 1,400
linear feet per day.

HEAVY EQUIPMENT OPERATOR
LINVILLE CREEK EXCAVATION LLC, MARION, NC | 2021 – 2023

· GPS Grade Control Monitors
· Scraper Operation
· Roller and Compactor Operation
· OSHA Trenching and Excavation Standards
· Preventive Maintenance
· Cut-and-Fill Calculations
· Soil Compaction Testing
· 
Loaded and relocated 1,870 cubic yards of rock and clay per shift using an excavator and off-road dump truck on a commercial pad preparation
site.
· Logged 37 survey hours per month assisting layout crews with grade stakes, cut sheets, and benchmark verification before each grading pass.
· Operated a roller compactor to compact subgrade in 6-inch lifts, achieving density readings confirmed by nuclear gauge testing within 22
minutes of each pass.
· Maintained 1 recordable incident across a full calendar year by following OSHA trenching and excavation standards during utility corridor work.



C E R T I F I C AT I O N S

EQUIPMENT OPERATOR TRAINEE
PISGAH HOLLOW SITE SERVICES INC., OLD FORT, NC | 2020 – 2021


· Commercial Driver's License (Class A), Home state driver
licensing agency, under FMCSA minimum standards, 2020
· 
Operated a backhoe to pull stumps and rip deteriorated asphalt on residential demolition sites, clearing an average of 1,130 square feet per
day.
· Completed 24 survey hours in the first 90 days by shadowing the site surveyor during control-point establishment and elevation checks.
· Performed pre-shift and post-shift fluid checks, greasing, and air-filter changes on a front-end loader and skid steer, cutting unplanned repair
calls from 5 per month to 1 per month over 8 months.





A.A.S. in Automotive Systems TechnologyE D U C AT I O N

Catawba Valley Community College, Hickory, NC | 2018 – 2020
image1.png




image2.png




image3.png
pal;




image4.png




